To install Levenhuk ToupView(R) software, please follow these steps:

1. For Windows OS:

- Run this file: autorun.exe.
- Click the "Install Image Software" button to install
Levenhuk ToupView(R) application for Windows.
- Click the "Advanced User Manual" button to view the
detailed user manual in English, or browse the CD.
- Click the "Basic User Manual" button to view the
QuickStart in Russian, or browse the CD.
- User Manual for your Levenhuk camera is available in the Manuals
folder.
- Click the "Install DirectShow Driver" button to install 
DirectShow driver for 3rd-party software or for development.
- Click the "Install Twain Driver" button to install Twain
driver for 3rd-party software or for development.  

2. For Mac OS:

- Locate the ToupViewX_Mac folder on your CD. Run the
ToupViewX.dmg file to install Levenhuk ToupViewX(R) application for Mac OS.
- The Manuals folder includes the detailed user manual in
English, the QuickStart in Russian and the user manual for
your Levenhuk camera.

3. For Linux:
- Locate the ToupViewX_Linux folder on your CD. Unpack the
ToupViewX.tar.gz file and run the installation file to install
Levenhuk ToupViewX(R) application for Linux.
- The Manuals folder includes the detailed user manual in
English, the QuickStart in Russian and the user manual for
your Levenhuk camera.

(c) 2006-2014 Levenhuk, Inc. USA
====